[bookmark: _GoBack]Table S1. Broflanilide (mg/m2) content on filter papers sprayed with VECTRON TM T500 and Primiphos-methyl (mg/m2) sprayed with Actellic 300CS on different wall surfaces of the experimental huts, Ethiopia 
	Vertical position on wall 
	VECTRON T500_HUT1
	VECTRON T500_HUT2
	VECTRON T500_HUT3

	
	Mud 
	Dung
	Paint
	Cement
	Mud 
	Dung
	Paint
	Cement
	Mud 
	Dung
	Paint
	Cement

	High
	12
	250
	152
	211
	162
	178
	201
	300
	160
	220
	210
	201

	Middle
	15
	160
	175
	160
	130
	210
	140
	275
	175
	170
	320
	342

	Low
	14
	150
	95
	110
	73
	151
	140
	230
	150
	200
	110
	210

	Vertical position on wall
	Actellic 300CS_HUT_1
	Actellic 300CS_HUT_2
	Actellic 300CS_HUT_3

	
	Mud 
	Dung
	Paint
	Cement
	Mud 
	Dung
	Paint
	Cement
	Mud 
	Dung
	Paint
	Cement

	High
	100
	1202
	1901
	1402
	1650
	2600
	2150
	1400
	700
	1900
	1900
	2001

	Middle
	650
	1501
	2750
	1250
	1850
	1950
	1700
	1500
	800
	1500
	1700
	1800

	Low
	700
	1200
	1600
	1070
	1250
	1300
	750
	1100
	950
	1700
	1570
	1649




