[bookmark: _GoBack]Table  10 Description and values of parameters used in health risk assessment equations
	Faktor
	Definition
	Unit
	Value
	Reference

	
	
	
	Adult
	Children
	

	C
	Metal concentration 
	mg kg−1
	–
	–
	-

	Ring
	Ingestion rate 
	mg day−1
	100
	200
	USEPA (2011)

	ED
	Exposure duration
	years
	24
	6
	USEPA (2002)

	EF
	Exposure frequency
	days year−1
	350
	350
	USEPA (1997)

	CF
	Conversion factor
	kg mg−1
	10E-06
	10E-06
	–

	BW
	Body weight
	kg
	70
	15
	USEPA (1997)

	AT
	Average time 
	years
	24
	6
	USEPA (2002)

	Cinh
	Inhalation rate 
	m3 day−1
	5
	20
	Du et al. (2013)

	PEF
	Particle emission factor
	m3 kg−1
	1.36E09
	1.36E09
	USEPA (2002)

	SA
	Skin surface area
	cm2
	5700
	2800
	USEPA (2002)

	SL
	Skin deference factor
	mg cm−2
	0.07
	0.07
	USEPA (2002)

	ABS
	Dermal absorption factor
	–
	0.01
	0.01
	USEPA (2011)

	RFD
	Reference dose
	mg kg−1  day−1
	Ing RFD
1.00E−03 (Cd), 5.00E−03 (Cr), 2.00E−02 (Co), 3.70E−02 (Cu), 2.00E−02 (Ni), 3.50E−03 (Pb), 3.00E−01 (Zn), 1.60E-04 (Hg)
Inh RFD
1.00E−03 (Cd), 2.86E−05 (Cr), 1.00E−02 (Co), 4.02E−02 (Cu), 2.06E−02 (Ni), 3.52E−03 (Pb), 3.00E−01 (Zn), 8.60E-03 (Hg)
Derm RFD
5.00E−05 (Cd), 2.50E−04 (Cr), 1.60E−02 (Co), 1.90E−03 (Cu), 1.00E−03 (Ni), 5.25E−04 (Pb), 6.00E−02 (Zn), 2.10E-05 (Hg)
	Abdelhafez et al. 2012;
Du et al. 2013; Tang et al.2020;
Ma et al 2018



