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Table (1) Water Zone Budgets

	Component
	Inflow (m3/day)
	% inflow
	Outflow (m3/day)
	%
Outflow
	Discrepancy
(m3/day)

	Recharge
	729810.94
	55.9
	-
	-
	

	Well discharge
	-
	
	704647.08
	54
	

	ET
	-
	
	50891.178
	3.9
	

	River leakage
	387761.84
	29.7
	22015.83
	1.6
	

	GHB
	187808.14
	14.4
	528485.31
	40.5
	

	Total
	1305381
	100
	1304902
	100
	478.88




Table(2) Summary of The Main Differences Among The Scenarios

	Growth Rate% of Wells' discharge
	Total Well Discharge(m3/d)
	Maximum Drawdown (m)
	Subsurface Inflow (m3/d)
	Subsurface Outflow (m3/d)

	20%
	36495.3
	13.382
	1308224.25
	1307740.75

	40%
	42577.98
	13.384
	1311070.25
	1310581.13

	60%
	48660.54
	13.386
	1313900
	1313420.50

	80%
	54743.15
	13.388
	1316745.63
	1316260.13

	100%
	60825.55
	13.390
	1319591.63
	1319100













Table (3) Shows The Difference In Static Water Level With Time

	Well name
	SWL(m)
	Q(m/d)
	Depth(m)
	Elevation a.m.s.l
	Time
	Distance (km)

	Dem-terafee
	20
	36.4
	133
	470
	1992
	

	Abd-elgabar
	34.2
	17
	130
	475
	2011
	4.3

	
	
	
	
	
	
	

	Zaydab
	14
	18.2
	193
	
	1993
	6

	Elgemma
	33
	17.3
	219
	489
	2011
	

	
	
	
	
	
	
	

	Elgoz
	18.9
	40.9
	136
	483
	1996
	5.6

	Aswan
	36.5
	
	274
	480
	2009
	

	
	
	
	
	
	
	

	Shendi
	15.8
	9
	109
	362
	2012
	

	Fazaab
	11
	22.7
	108
	360
	2005
	2.7

	
	
	
	
	
	
	

	Alkhraba
	15
	40
	106
	430
	2004
	

	Algood
	26.6
	13.6
	220
	426
	2013
	13.5

	

	
	
	
	
	
	

	Awlad-nasar
	16.8
	32.7
	146
	398
	1988
	10.3

	Raya
	34.2
	14.2
	201
	410
	2009
	




