Online Resource Table 1 Class-level landscape metrics for the 5 land cover classifications, that were extracted from clipped buffers surrounding camera sites at 200m, 500m, 1km, and 2km using FRAGSTATS version 4
	Class-level Landscape Metrics 
	Definition
	Unit

	Percentage of Landscape (PLAND)
	Equals the percentage of the landscape that is made up of that patch type.
	Percent

	Patch Area (AREA_MN)
	In class, it is the function of number of patches and total class area. It represents the average condition.
	ha

	Edge Density (m/ha) (ED)
	The ratio between edge length and per unit area. 
	Meters per hectare

	Patch Density (PD)
	Calculates number of patches per unit
	Number per hectares

	Patch Cohesion Index (COHESION)
	At class level, it measures the physical connectedness of the patch type
	None

	Largest Patch Index (LPI)
	Quantifies the percentage of total landscape area made by the largest patch
	Percent




