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[image: ]Figure S.1. Particles size distribution of Pt/Ta2O5-La/MWCNTs

Figure [image: ]S.2. Schematic diagram of the electrochemical test setup


[bookmark: _Hlk174434688][image: ]Figure S3. CV curves(current per electrochemically active surface area of Pt) of Pt/Ta2O5-La/MWCNTs catalysts with 15%, 20%, 25%, and 30% La content and Pt/Ta2O5/MWCNTs in 0.5 M H2SO4 + 1 M CH3OH solution at a scan rate of 50 mV s-1.
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Figure S.4. CO-stripping curves of Pt/Ta2O5-La/MWCNTs catalysts with 15%, 20%, 25%, and 30% La content in 0.5 M H2SO4 at a scan rate of 50 mV s-1 and under potential of -0.25V to 1V.
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