Supplementary Information

Power spectrum curves for 250 nm beads with corresponding Lorentzian fits
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Power spectrum curves for 500 nm beads with corresponding Lorentzian fits
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Power spectrum curves for 1 µm beads with corresponding Lorentzian fits
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