Table 1 Lighting scenes and spectral power distribution of 3 lighting groups
	Lighting parameters
	Lighting scenes
	Spectral power distribution (SPD)

	(WLG)
3000 K 
500 lx
	[image: A hospital room with a bed and a window

Description automatically generated]
	[image: A diagram of a spectrum

Description automatically generated]

	(CG)
5000 K
500 lx
	[image: A hospital room with a hospital bed

Description automatically generated]
	[image: A graph of a spectrum

Description automatically generated]

	(CLG)
6500 K
500 lx
	[image: A hospital room with a bed and a window

Description automatically generated]
	[image: A graph showing a spectrum of colors

Description automatically generated]

	(Normal)
3500 K
166 lx
	[image: A group of people in a room

Description automatically generated]
	[image: A diagram of a spectrum

Description automatically generated]
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