High performance nanoplasmonic UV/VIS/NIR photodetector fabricated in ambient condition
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Figure S1: (a) SiNWs covered by dendrite layers of Ag, (b) Optical reflectance of SiNWs arrays covered with dendrite layers of Ag.
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Figure S2: Stability measurement of the signal before the I-T measurements.
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