Development and Validation of a Model for Soil Wetting Geometry under Moistube Irrigation
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Appendix I
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Figure 9 Soil matric – volumetric soil water content conversion chart for the silty clay loam soil
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