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Fig. S1. Morphologies of printed features at different frequencies with a pulse width of 5ms: (a) 100 Hz; (b) 140 Hz.
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Fig. S2. Morphologies of printed features at different frequencies with a pulse width of 0.2 ms:  (a) 40 Hz; (b) 80 Hz; (c) 160 Hz; (d) 320 Hz.
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