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	Figure S1: EDX of (a) bare substrate before CVD deposition and (b) As-grown monolayer WS2 on substrate after CVD deposition
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Figure S2: AFM operation on identified monolayer WS2
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