@inproceedings{srawley1976wide,
  title={Wide range stress intensity factor expressions for ASTM E 399 standard fracture toughness specimens},
  author={Srawley, John E},
  booktitle={Conf. of Am. Soc. for Testing and Mater., Committee E-24},
  note={E-8654},
  year={1976}
}

@article{qiao2019strength,
  title={Strength and cohesive behavior of thermoset polymers at the microscale: A size-effect study},
  author={Qiao, Yao and Salviato, Marco},
  journal={Engineering Fracture Mechanics},
  volume={213},
  pages={100--117},
  year={2019},
  publisher={Elsevier}
}

@book{BazantBook2021,
    author = {Bažant, Zdenek P. and Le, Jia-Liang and Salviato, Marco},
    title = {Quasibrittle Fracture Mechanics and Size Effect: A First Course},
    publisher = {Oxford University Press},
    year = {2021},
    month = {11},
    isbn = {9780192846242},
    doi = {10.1093/oso/9780192846242.001.0001},
    url = {https://doi.org/10.1093/oso/9780192846242.001.0001},
    eprint = {https://academic.oup.com/book/41613/book-pdf/50129547/9780192661388\_web.pdf},
}

@book{british2014method,
  title={Method of test for determination of fracture toughness in metallic materials using single edge notched tension (SENT) specimens},
  author={British Standards Institution},
  year={2014},
  publisher={British Standards Institution}
}

@article{tankasala2020crack,
  title={The crack growth resistance of an elastoplastic lattice},
  author={Tankasala, Harika C and Fleck, Norman A},
  journal={International Journal of Solids and Structures},
  volume={188},
  pages={233--243},
  year={2020},
  publisher={Elsevier}
}

@article{MEFFORD2017961,
title = {Failure behavior and scaling of graphene nanocomposites},
journal = {Composite Structures},
volume = {176},
pages = {961-972},
year = {2017},
issn = {0263-8223},
doi = {https://doi.org/10.1016/j.compstruct.2017.06.013},
url = {https://www.sciencedirect.com/science/article/pii/S0263822317307122},
author = {Cory Hage Mefford and Yao Qiao and Marco Salviato},
keywords = {Graphene, Fracture, Size effect, Damage}
}

@article{QIAO2019127,
title = {Study of the fracturing behavior of thermoset polymer nanocomposites via cohesive zone modeling},
journal = {Composite Structures},
volume = {220},
pages = {127-147},
year = {2019},
issn = {0263-8223},
doi = {https://doi.org/10.1016/j.compstruct.2019.03.092},
url = {https://www.sciencedirect.com/science/article/pii/S0263822318325789},
author = {Yao Qiao and Marco Salviato}
}

@article{CUSATIS20092163,
title = {Cohesive crack analysis of size effect},
journal = {Engineering Fracture Mechanics},
volume = {76},
number = {14},
pages = {2163-2173},
year = {2009},
issn = {0013-7944},
doi = {https://doi.org/10.1016/j.engfracmech.2009.06.008},
url = {https://www.sciencedirect.com/science/article/pii/S0013794409001921},
author = {Gianluca Cusatis and Edward A. Schauffert},
keywords = {Quasi-brittle fracture, Fracture energy, Size effect, Cohesive crack law, Concrete}
}

@article{10.1115/1.2806812,
author = {Bazˇant, Zdeneˇk P. and Daniel, Isaac M. and Li, Zhengzhi},
title = {Size Effect and Fracture Characteristics of Composite Laminates},
journal = {Journal of Engineering Materials and Technology},
volume = {118},
number = {3},
pages = {317-324},
year = {1996},
month = {07},
issn = {0094-4289},
doi = {10.1115/1.2806812},
url = {https://doi.org/10.1115/1.2806812},
eprint = {https://asmedigitalcollection.asme.org/materialstechnology/article-pdf/118/3/317/5717170/317_1.pdf},
}

@article{SALVIATO201667,
title = {Experimental and numerical investigation of intra-laminar energy dissipation and size effect in two-dimensional textile composites},
journal = {Composites Science and Technology},
volume = {135},
pages = {67-75},
year = {2016},
issn = {0266-3538},
doi = {https://doi.org/10.1016/j.compscitech.2016.08.021},
url = {https://www.sciencedirect.com/science/article/pii/S0266353816303384},
author = {Marco Salviato and Kedar Kirane and Shiva {Esna Ashari} and Zdeněk P. Bažant and Gianluca Cusatis},
keywords = {Textile composites, Non-linear fracture mechanics, Damage mechanics, Size effect, Two-dimensional composites, Microplane model}
}