Disagreement between anterior segment optical coherence tomography devices in eyes with a shallow anterior chamber
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Supplemental fig. 2 Iris-related parameters: A (IT750), B (IT2000), C (ICURVE), and D (IAREA). Legend: IT750 and IT2000 = iris thickness at 750 μm and 2000 μm from the scleral spur; ICURVE = iris curvature; IAREA = iris area.
Note: In all graphs, the data are distributed according to the difference between the measurements obtained with the two devices (y-axis: Visante® OCT – DRI OCT Triton®) and the mean of the values obtained (x-axis). The larger diamond represents patients for whom both devices assigned a value of zero to the variable. The solid line represents the mean difference between measurements and the dashed lines represent the limits of agreement.
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