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Figure S1: Preparation of TENG by varying concentrations of BTO in PDMS solution.
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Figure S2: Preparation of TENG by using Nylon as electronegative material.
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Figure S3: Preparation of TENG by using different molds for surface roughness.
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