Highlights
1. [bookmark: _GoBack]Hydrodynamic transport controls FPV fire-derived pollutant dispersion. 
2. EFDC+ resolves dilution, mixing, and receptor-level exposure. 
3. AIoT indicators constrain uncertainty in emission scaling. 
4. Transient concentration peaks dominate short-term exposure. 
5. Results support screening-level environmental assessment.

