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	Manufacturer
	Siemens Healthineers, Munich, Germany
	Siemens Healthineers, Munich, Germany

	Scanner Type
	SOMATOM Definition AS 
	SOMATOM Force

	Reconstruction kernel
	Br 38
	Br 40

	Slice thickness (mm)
	3.0
	3.0

	Iterative reconstruction algorithm
	Sinogram affirmed iterative reconstruction (SAFIRE), level 3
	Advanced modelled iterative reconstruction (ADMIRE), level 3

	Tube current-time product (mAs)
	190
	150

	Tube voltage (kV)
	120
	120

	Dose optimization
	Optimized for parenchymal scanning
	Optimized for parenchymal scanning

	Rotation time
	0.5 seconds
	0.5 seconds

	Contrast medium
	Ultravist 300
	Ultravist 300

	Maximum flow rate
	4.4 mL/s
	4.4 mL/s

	Injection duration (s)
	30 
	30

	Total contrast dose
	4 mL/kg, maximum 133 mL
	4 mL/kg, maximum 133 mL


Abbreviations: Br: body kernel, kg: kilograms, kV: kilovolts, mAs: milliampere seconds mL: millilitres, mm: millimetres, s: seconds

Supplementary material: 


 


Table 1: 


Scanner protocols used for the CT


-


abdomens


 


Manufacturer


 


Siemens Healthineers


, 


Munich, Germany


 


Siemens Healthineers


, 


Munich, Germany


 


Scanner Type


 


SOMATOM Definition AS 


 


SOMATOM Force


 


Reconstruction kernel


 


Br 38


 


Br 40


 


Slice thickness (mm)


 


3.0


 


3.0


 


Iterative reconstruction 


algorithm


 


Sinogram affirmed iterative 


reconstruction (SAFIRE), level 


3


 


Advanced mode


l


led iterative 


reconstruction (ADMIRE), 


level 3


 


Tube current


-


time product 


(mAs)


 


190


 


150


 


Tube voltage 


(kV)


 


120


 


120


 


Dose optimization


 


Optimized for parenchymal 


scanning


 


Optimized for parenchymal 


scanning


 


Rotation time


 


0.5 seconds


 


0.5 seconds


 


Contrast medium


 


Ultravist 300


 


Ultravist 300


 


Maximum flow rate


 


4.4 mL/s


 


4.4 mL/s


 


Injection duration


 


(s)


 


30 


 


30


 


Total contrast dose


 


4 mL/kg, maximum 133 mL


 


4 mL/kg, maximum 133 mL


 


Abbreviations: Br: body kernel, kg: kilograms, kV: kilovolts, mAs: mil


l


iampere seconds 


mL: 


millilitres


,


 


mm: millimetres, 


s: seconds


 




Supplementary material:    Table 1:  Scanner protocols used for the CT - abdomens  

Manufacturer  Siemens Healthineers ,  Munich, Germany  Siemens Healthineers ,  Munich, Germany  

Scanner Type  SOMATOM Definition AS   SOMATOM Force  

Reconstruction kernel  Br 38  Br 40  

Slice thickness (mm)  3.0  3.0  

Iterative reconstruction  algorithm  Sinogram affirmed iterative  reconstruction (SAFIRE), level  3  Advanced mode l led iterative  reconstruction (ADMIRE),  level 3  

Tube current - time product  (mAs)  190  150  

Tube voltage  (kV)  120  120  

Dose optimization  Optimized for parenchymal  scanning  Optimized for parenchymal  scanning  

Rotation time  0.5 seconds  0.5 seconds  

Contrast medium  Ultravist 300  Ultravist 300  

Maximum flow rate  4.4 mL/s  4.4 mL/s  

Injection duration   (s)  30   30  

Total contrast dose  4 mL/kg, maximum 133 mL  4 mL/kg, maximum 133 mL  

Abbreviations: Br: body kernel, kg: kilograms, kV: kilovolts, mAs: mil l iampere seconds  mL:  millilitres ,   mm: millimetres,  s: seconds  

