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Impact of Debris Accumulation Length on Hydraulic
Performance of Trash Screens in Open Channels
Accumulation Length Matters Beyond Blockage Ratio
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