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[bookmark: OLE_LINK61][bookmark: OLE_LINK64]sFig.1. Simulation Results of Bending Deformation of Photovoltaic Modules with Glass Fiber Reinforced Plastic Frames at Different Temperatures (2.5mm).
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[bookmark: OLE_LINK62]sFig.2. Simulation Results of Bending Deformation of Photovoltaic Modules with Carbon Fiber Reinforced Plastic Frames at Different Temperatures (2.5mm).
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[bookmark: OLE_LINK63]sFig.3. Simulation Results of Bending Deformation of Photovoltaic Modules with Al Frames at Different Temperatures (2.5mm). 
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[bookmark: OLE_LINK65]sFig.4. Simulation Results of Bending Deformation of Photovoltaic Modules with Glass Fiber Reinforced Plastic Frames at Different Temperatures (2.5mm) under a load of 2.4kPa. 
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[bookmark: OLE_LINK66]sFig.5. Simulation Results of Bending Deformation of Photovoltaic Modules with Carbon Fiber Reinforced Plastic Frames at Different Temperatures (2.5mm) under a load of 2.4kPa. 
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sFig.6. Simulation Results of Bending Deformation of Photovoltaic Modules with Al Frames at Different Temperatures (2.5mm) under a load of 2.4kPa. 
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