Novelty Statement
In the present article, the effect of different vol % of Ni doped TiO2 thin films on structural, microstructural, electrical, optical and humidity sensing properties were investigated. Pristine and Ni doped TiO2 thin films were synthesized using spray pyrolysis technique. The maximum humidity sensitivity of 89% was observed for the sample with 2 vol% of Ni doped TiO2 with low response time of 64 s.
