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Figure Captions
Fig. S1 DTG and TGA curves of the samples collected at different times of the composting process: (a) Tl and DS; (b-d) FM, MM, and CM on D0 and D40.

Table S1 Physicochemical characteristics of the raw materials.
	Characteristics
	Feedstocks

	
	Dewatered sludge
	Triarrhena lutarioriparia
	FM
	MM
	CM

	Moisture content (wet basis %)
	78.9
	9.63
	54.6
	57.3
	50

	Organic matter (dry basis %)
	45.1
	95.8
	86.1
	85.9
	87.1

	pH
	7.04
	6.53
	7.18
	7.19
	7.30

	EC (mS/cm)
	0.54
	2.74
	2.23
	3.07
	2.37

	TN (%)
	3.7
	1
	1.46
	1.54
	1.58

	TP (%)
	4.64
	0.27
	1.71
	1.95
	1.31

	TK (%)
	1.85
	1.62
	1.81
	1.92
	1.61

	DOC (mg/L)
	590.0
	491.6
	876.3
	878.4
	906.6



Table S2 Evaluation of GI, HA, and FA value for FM, MM and CM on D0 and D40.
	Compost
	Stage
	GI (%)
	HA (mg/g)
	FA (mg/g)

	FM
	0
	62.43
	97.6
	43.05

	
	40
	116.65
	167.55
	37.7

	MM
	0
	58.62
	97.71
	44.82

	
	40
	110.89
	162.93
	38.64

	CM
	0
	65.44
	93.32
	46.13

	
	40
	65.83
	133.07
	43.58





Table S3 Evolution of the humification ratios for FM, MM and CM on D0 and D40.
	Compost
	Stage
	1643/2919
	1643/2840
	1525/2919
	1425/1050

	FM
	0
	0.85
	0.72
	1.10
	2.43

	
	40
	0.72
	0.63
	0.99
	3.17

	MM
	0
	0.97
	0.82
	1.28
	1.97

	
	40
	0.80
	0.73
	1.02
	2.30

	CM
	0
	0.83
	0.71
	1.10
	2.75

	
	40
	0.83
	0.75
	1.04
	1.96



Table S4 Changes of heavy metal concentration before and after composting in three piles.
	Compost
	Stage
	Cd(mg/kg)
	Cr(mg/kg)
	Cu(mg/kg)
	Ni(mg/kg)
	Pb(mg/kg)
	Zn(mg/kg)

	FM
	D0
	0.71
	36.14
	64.02
	11.65
	12.57
	302.91

	
	D8
	0.47
	40.61
	63.98
	14.56
	13.89
	331.83

	
	D40
	0.45
	42.77
	70.38
	16.49
	14.07
	353.10

	MM
	D0
	0.61
	33.79
	62.23
	11.46
	11.40
	296.04

	
	D8
	0.40
	40.49
	64.60
	15.18
	11.64
	354.00

	
	D40
	0.49
	49.37
	75.24
	18.13
	13.52
	384.67

	CM
	D0
	0.58
	43.83
	71.04
	15.66
	14.23
	326.64

	
	D8
	0.38
	34.38
	56.37
	12.90
	9.72
	294.64

	
	D40
	0.25
	34.33
	59.22
	13.02
	8.66
	307.67
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Fig. S1 DTG and TGA curves of the samples collected at different times of the composting process: (a) Tl and DS; (b-d) FM, MM, and CM on D0 and D40.
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