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Highlights 
· Coupling biosorption with anodic oxidation offers high efficiency at low energy consumption when degrading Amaranth Red (E123) 
· Coupling process  is proved to be effective for the enhancement of the stability of SS/PbO2 anodes 
· Luffa cylindrica  ability for reuse was confirmed after three regeneration cycles
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