Highlights

Composting cells with perforated walls (CCPW) are efficient in static piles
CCPW are efficient to dispense the aeration during composting of hatchery waste
During the winter the low air humidity slows down the biodegradation process
Biodegradation during the composting was influenced for the air humidity variations

