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	T1-weighted image
	diffusion weighted image

	Manufacturer
	Siemens 3T TrioTim
	Siemens 3T TrioTim

	Repetition time (ms)
	2300
	9200

	Echo time (ms)
	2.98
	82

	Slice Thickness (mm)
	1
	2.7

	Voxel size
	1 x 1 x 1
	2.73 x 2.73 x 2.73

	b-value (s/mm2)
	-
	1000

	directions
	-
	44

	Phase encoding direction
	-
	Anterior-Posterior

	
	
	


[bookmark: OLE_LINK423][bookmark: OLE_LINK424]Abbreviations: mm = mulimeters; ms = miliseconds; s = seconds.

