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[bookmark: _GoBack]Corrosion inhibitor TZBM effectively slows down the corrosion of carbon steel in 180℃ solutionliquid containing Cl-+H2S+CO2.
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