[bookmark: _GoBack]Table 3. Reduction Rate (%) of PM10, PM2.5, HCHO, TVOC, and CO2 by indoor plants
	Indoor Pollutant
	Apartment

	Condition
	Mean±SE
	Reduction Rate (%)

	PM10
	Apartment I (APT I)
Apartment II (APT II)
Apartment III (APT III)
Apartment IV (APT IV)
	Ventilation ✔ & Indoor plant (C3+CAM) ✔
Ventilation ✘ & Indoor plant (CAM) ✔
Ventilation ✔ & Indoor plant ✘
Ventilation ✘ & Indoor plant ✘
	19.4±0.74
21.82±0.21
29.02±0.94
58.81±1.66
	67.01%                                                                 62.89%
50.65%.
Control

	PM2.5
	Apartment I (APT I)
Apartment II (APT II)
Apartment III (APT III)
Apartment IV (APT IV)
	Ventilation ✔ & Indoor plant (C3+CAM) ✔
Ventilation ✘ & Indoor plant (CAM) ✔
Ventilation ✔ & Indoor plant ✘
Ventilation ✘ & Indoor plant ✘
	12.64±0.32
17.11±0.13
15.94±0.5
35.72±0.96
	
64.61%                                                                 52.09%
56.63%                                                                       Control.


	TVOC
	Apartment I (APT I)
Apartment II (APT II)
Apartment III (APT III)
Apartment IV (APT IV)
	Ventilation ✔ & Indoor plant (C3+CAM) ✔
Ventilation ✘ & Indoor plant (CAM) ✔
Ventilation ✔ & Indoor plant ✘
Ventilation ✘ & Indoor plant ✘
	56.35±6.59
190.93±7.63
84.42±3.03
800.41±14.73
	
92.95%                                                               76.14%
89.41%                                                                       Control.


	HCHO
	Apartment I (APT I)
Apartment II (APT II)
Apartment III (APT III)
Apartment IV (APT IV)
	Ventilation ✔ & Indoor plant (C3+CAM) ✔
Ventilation ✘ & Indoor plant (CAM) ✔
Ventilation ✔ & Indoor plant ✘
Ventilation ✘ & Indoor plant ✘
	6.023±0.255
5.98±0.06
34.67±0.35
23.99±0.32
	

74.89%                                                                 75.07%
-30%                                                                       Control



	CO2
	Apartment I (APT I)
Apartment II (APT II)
Apartment III (APT III)
Apartment IV (APT IV)
	Ventilation ✔ & Indoor plant (C3+CAM) ✔
Ventilation ✘ & Indoor plant (CAM) ✔
Ventilation ✔ & Indoor plant ✘
Ventilation ✘ & Indoor plant ✘
	615.5±2.73
1154.52±10.83
1278.42±9.27
2616.36±25.81
	
76.47%                                                                 55.87%
51.13%                                                                       Control.



Values are means ± SE; (p < 0.0005); (p < 0.0001); (p > 0.0005)

