[bookmark: _Ref51687656][bookmark: _Toc40712994]Table 5: Measured displacements, strains and Poisson’s ratio of auxetic composite in the case of tensile test
	∆L
	∆T
	
	
	

	20
	13.52
	0.028
	0.080
	- 2.86



[bookmark: _Ref51692622]Table 6: Measured displacements, strains and Poisson’s ratio of honeycomb composite in the case of tensile test
	∆L
	∆T
	
	
	

	15
	- 24.61
	0.019
	- 0.154
	8.10




[bookmark: _Ref40408644][bookmark: _Toc40712996]Table 7: Measured displacements, strains and Poisson’s ratio of auxetic composite in the case of compression test
	∆h
	∆d
	
	
	

	- 20.04
	- 10.1
	0.014
	0.118
	- 0.12




[bookmark: _Ref51695360][bookmark: _Ref51695281]Table 8: Measured displacements, strains and Poisson’s ratio of honeycomb composite in the case of compression test
	∆h
	∆d
	
	
	

	- 20.06
	10
	- 0.125
	0.118
	0.11





