Highlights

· Optimization using Response Surface Methodology is by Central Composite Design.
· BHA brings out the better performance of natural esters than the BHT.
· Higher the antioxidant content will increase the conductivity in oil.
· Natural esters and antioxidants added blended natural esters are the appropriate choice of alternate insulating medium for better performance.

