Highlights
Dunaliella salina and Porphyridium cruentum were cultivated in pilot scale tubular photobioreactor
Spray drying technique as used to prepare dried biomass.
The biomass were encapsulated by using spray-drying and RSM I-optimal methods
Total carotenoid, Chlorophyll-a and moisture contents were modelled significantly
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