Highlights for manuscript Joining of cemented carbides WC-Co and tool steel X153CrMoV12 with capacitor discharge welding process 

· At multi-CD welding of cemented carbides and tool steel a molten phase is formed.
· The zone with chromium depletion and mixed layer are formed in the joining zone.
· The molten phase is pushed out of join as bead with dendritic structure Cr enriched.
