Highlights
· The geomechanical properties of Middle Jurassic reservoirs have been identified.
· Distribution of resistive and conductive fractures are controlled by the stress regimes. 
· Minimum horizontal stress (SHmin) and breakout directions are structurally-controlled. 
· [bookmark: _GoBack]Fracture analysis reveals two natural fractures induced by critically stress regimes.

