Table 1. The key features and drawbacks of developed liver-on-a-chip systems.
	
	Design
	Key features
	Drawbacks

	v1
	[image: Paveikslėlis, kuriame yra tekstas

Automatiškai sugeneruotas aprašymas]
	· Tesla valve
· μm scale channels
· Small volumes of substances required
· 1 cm length reaction zone
	· Sharp corners
· Long filling lines
· Complicated filling procedure due to undesired air bubbles

	v2
	[image: Paveikslėlis, kuriame yra tekstas

Automatiškai sugeneruotas aprašymas]
	· μm scale channels
· Small volumes of substances required
· 1 cm length reaction zone
	· Sharp corners
· Long filling lines
· Complicated filling procedure due to undesired air bubbles

	v3
	[image: ]
	· Tesla valve - stops substances flowing out of the chip.
· μm scale channels
· Small volumes of substances required.
· 1 cm length reaction zone
	· Sharp corners
· Long filling lines
· Complicated filling procedure due to undesired air bubbles

	v4
	[image: ]
	· Short filling channels
· Wide filling ports
· Short filling lines
· Smooth edges, no dead ends or microwells
	· Shorter 5 mm reaction zone
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