Highlights:
· An energy-based design procedure applicable to the Chinese code is proposed for self-centering shear wall systems.
· The controllability of the damage development in designed structures can be achieved by assigning rational damage indexes in the procedure.
· The procedure allows designers to perform multi-level designs by selecting various performance objectives under different seismic levels.
