	Mooring
	Location
	Water Depth [m]
	Instrument
	Height of Most Proximal Data Above Bed [m]
	Height of Most Distal Data Above Bed [m]
	Bin size [m]
	Deployment Date
	Recovery Date

	C02
	Open Slope
	1768
	Aanderaa Seaguard Current Meter
	3 & 5
	
	
	2013-03-11
	2014-10-25

	C03A
	Tungue Canyon
	1014
	Aanderaa Seaguard Current Meter
	3 & 5
	
	
	2013-03-11
	2014-04-20

	C03B
	Tungue Canyon
	1710
	Aanderaa Seaguard Current Meter
	3 & 5
	
	
	2014-04-25
	2014-10-25

	C04
	Open Slope
	993
	Aanderaa Seaguard Current Meter
	3 & 5
	
	
	2013-03-11
	2014-10-26

	C05A
	Tungue Canyon
	603
	Upward-looking RDI 300 kHz ADCP
	15
	111
	2
	2013-03-12
	2013-12-04

	
	
	
	Aanderaa Seaguard Current Meter
	3 & 5
	
	
	
	

	C05B
	Open Slope
	595
	Upward-looking RDI 300 kHz ADCP
	15
	113
	2
	2013-12-05
	2014-10-25

	
	
	
	Aanderaa Seaguard Current Meter
	3 & 5
	
	
	
	

	C06
	Open Slope
	199
	Aanderaa Seaguard Current Meter
	3 & 5
	
	
	2013-03-09
	2014-10-26

	C08
	Open Slope
	520
	Aanderaa Seaguard Current Meter
	3 & 5
	
	
	2013-03-10
	2014-10-26

	C09B
	Afungi Canyon
	1822
	Aanderaa Seaguard Current Meter
	3 & 5
	
	
	2014-04-27
	2014-10-25

	C11B
	Mebuisi Canyon
	1506
	Aanderaa Seaguard Current Meter
	3 & 5
	
	
	2014-04-26
	2014-10-25

	C12
	Open Slope
	197
	Aanderaa Seaguard Current Meter
	3 & 5
	
	
	2013-03-09
	2014-10-25

	CM06A
	Tungue Canyon Head
	116
	Downward-looking 600 kHz ADCP
	10.5
	21
	0.5
	2011-12-23
	2012-04-26

	CM06B
	Vamizi Canyon
	1126
	Downward-looking 600 kHz ADCP
	10.5
	20
	0.5
	2012-10-05
	2015-03-31

	CM08A
	Open Slope
	686
	Downward-looking 600 kHz ADCP
	10.5
	23
	0.5
	2011-12-24
	2012-05-05

	CM08B
	Open Slope
	1531
	Downward-looking 600 kHz ADCP
	10.5
	15
	0.5
	2011-09-29
	2015-01-15

	CM09A
	Afungi Canyon
	431
	Downward-looking 600 kHz ADCP
	10.5
	21.5
	0.5
	2011-12-24
	2013-02-05

	CM09B
	Afungi Canyon
	948
	Downward-looking 600 kHz ADCP
	10.5
	20
	0.5
	2013-02-10
	2013-05-10

	CM09C
	Afungi Canyon
	449
	Downward-looking 600 kHz ADCP
	10.5
	18
	0.5
	2013-09-07
	2014-07-01

	CM10
	Gully
	546
	Downward-looking 600 kHz ADCP
	10.5
	16.5
	0.5
	2012-09-27
	2015-03-31

	CM11
	Tungue Canyon
	1583
	Downward-looking 600 kHz ADCP
	10.5
	15
	0.5
	2011-12-25
	2015-04-02

	CM12A
	Afungi Canyon
	1842
	Downward-looking 600 kHz ADCP
	10.5
	17
	0.5
	2011-12-25
	2012-04-02

	CM12B
	Afungi Canyon
	1766
	Downward-looking 600 kHz ADCP
	10.5
	13.5
	0.5
	2012-10-04
	2015-03-29

	CM13A
	Open Slope
	1503
	Downward-looking 600 kHz ADCP
	10.5
	17
	0.5
	2012-09-29
	2013-06-26

	CM13B
	Open Slope
	1521
	Downward-looking 600 kHz ADCP
	10.5
	16
	0.5
	2013-11-16
	2015-04-01

	CM15
	Gully
	1572
	Downward-looking 600 kHz ADCP
	10.5
	19
	0.5
	2013-02-05
	2015-01-17

	CM16
	Vamizi Canyon
	1811
	Downward-looking 600 kHz ADCP
	10.5
	17.5
	0.5
	2013-02-04
	2015-03-31

	D1
	Gully 
	717
	Downward-looking 600 kHz ADCP
	11
	35
	1
	2014-07-28
	2015-04-18

	D2
	Gully 
	1213
	Downward-looking 600 kHz ADCP
	11
	34
	1
	2014-07-27
	2015-04-16

	D3
	Mebuisi Canyon
	923
	Downward-looking 600 kHz ADCP
	11
	36
	1
	2014-07-21
	2015-04-18

	D4
	Open Slope
	249
	Downward-looking 600 kHz ADCP
	11
	38
	1
	2014-07-20
	2015-04-20

	D5
	Mebuisi Canyon
	1606
	Downward-looking 600 kHz ADCP
	11
	30
	1
	2014-07-26
	2015-04-15

	D6
	Gully
	1522
	Downward-looking 600 kHz ADCP
	11
	28
	1
	2014-07-27
	2015-04-14

	D7
	Gully
	996
	Downward-looking 600 kHz ADCP
	11
	35
	1
	2014-07-20
	2015-04-17

	D8
	Tungue Canyon
	746
	Downward-looking 600 kHz ADCP
	11
	34
	1
	2014-07-21
	2015-04-20


Table S1. Specifications and location information for the moorings and instruments deployed offshore North Mozambique.
