[bookmark: _GoBack]Supplementary Table 3 GCI results for the different CFD metrics of average and maximum wall shear stress (WSS) across the entire geometry, as well as mass flow rates (MFR) for the left (ICAL) and right (ICAR) internal carotid, left (VAL) and right (VAR) vertebral and left (CRAL) and right (CRAR) central retinal arteries respectively. CFD metrics were obtained at steady systole flow conditions.
	CFD Metric
	GCI

	Average WSS (Pa)
	0.10%

	Max WSS (Pa)
	1.95%

	MFR ICAL (kg/s)
	2.59%

	MFR VAL (kg/s)
	0.01%

	MFR ICAR (kg/s)
	0.05%

	MFR VAR (kg/s)
	0.22%

	MFR CRAL (kg/s)
	0.12%

	MFR CRAR (kg/s)
	0.09%



