Graphical Abstract
In this work, NR/MXene/SiO2 nanocomposites are fabricated into flexible wearable strain sensors with an island-chain structure, this unique structure promotes the selective distribution of MXene in the NR matrix and greatly improves the sensing performance of the material, which can detect human motions in real-time and provide personal health monitoring.
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