Computational study of the performance of a solar dryer for improvement in the shelf life of the food materials
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Highlights:
· A thermal model of fabricated indirect type solar dryer has been developed.
· Model equations have been solved in the MATLAB environment.
· Experimental work has been performed in fabricated solar dryer.
· Thermal efficiency of the dryer was found 53.7 %.
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