Table 4. Value of movement velocity of tested GNSS stations
	No
	[bookmark: _GoBack]Stations
	V (mm/yr)
	V calculated from the model (mm/yr)
	Deviation (mm/yr)

	1
	OAN0
	35.12
	37.03
	-1.91

	2
	LOT1
	35.62
	35.58
	0.04

	3
	C075
	37.30
	35.30
	2.00
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