High lights

1. A T-SVE apparatus with a large heating cylinder was constructed.
2. Thermal conductivity was a crucial factor influencing remediation efficiency.
3. Volatilization of n-alkanes from heated soils showed an irregular pulsed mode. 
4. Soil organic matter exhibited a trivial impact on heat transfer behavior in soils.
5. Higher soil moisture firstly retarded and then accelerated the removal of n-alkanes.

