Highlights
· The catalyst coating effectively increased the discharge intensity of the DBD system.
· N atoms were incorporated into the TiO2 crystal lattice, replacing some O atoms.
· Hydroxyl groups on the catalyst coating surface facilitated O3 synthesis.
· [bookmark: _GoBack]The catalyst coating facilitated the generation of catalytic sites for O3 synthesis.

