Highlight for Reviewers

1- Nanocomposite films consisting of polystyrene (PS) doped with concentrations 2, 4, 6, 8 and 10 wt% nickel (II) oxide (NiO) nanoparticles were prepared by casting technique and studied by XRD; SEM and FT-IR.
2- The optical and Conductivity of PS/NiO (NCs) films were studied. 
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