Supplementary Data
Table S1 The flow rates of eight tested light-duty vehicle
	No
	flow rate (m3/min)
	No
	flow rate (m3/min)

	No.1
	8.92
	No.5
	8.95

	No.2
	8.92
	No.6
	8.98

	No.3
	8.96
	No.7
	8.64

	No.4
	8.95
	No.8
	8.77


Table S2 The ratio of four conditions under WLTC and CLTC-P
	No
	Test cycle
	WLTC
	CLTC-P

	
	Characteristic
	Idle Ratio
	Acceleration Ratio
	Deceleration Ratio
	Cruise Ratio
	Idle Ratio
	Acceleration Ratio
	Deceleration Ratio
	Cruise Ratio

	
	Unit
	%
	%
	%
	%
	%
	%
	%
	%

	No.1
	Total
	0.12 
	0.33 
	0.34 
	0.21 
	0.22 
	0.33 
	0.31 
	0.14 

	
	Low Speed
	0.24 
	0.29 
	0.37 
	0.10 
	0.35 
	0.27 
	0.24 
	0.13 

	
	Medium Speed
	0.11 
	0.37 
	0.34 
	0.19 
	0.19 
	0.34 
	0.32 
	0.14 

	
	High Speed
	0.06 
	0.32 
	0.29 
	0.33 
	0.05 
	0.41 
	0.37 
	0.17 

	No.2
	Total
	0.13 
	0.34 
	0.33 
	0.20 
	0.21 
	0.32 
	0.31 
	0.16 

	
	Low Speed
	0.25 
	0.28 
	0.35 
	0.11 
	0.34 
	0.24 
	0.23 
	0.18 

	
	Medium Speed
	0.11 
	0.40 
	0.34 
	0.15 
	0.19 
	0.34 
	0.34 
	0.12 

	
	High Speed
	0.06 
	0.31 
	0.31 
	0.32 
	0.05 
	0.42 
	0.36 
	0.17 

	No.3
	Total
	0.13 
	0.33 
	0.33 
	0.21 
	0.22 
	0.33 
	0.29 
	0.16 

	
	Low Speed
	0.25 
	0.29 
	0.35 
	0.11 
	0.35 
	0.26 
	0.23 
	0.15 

	
	Medium Speed
	0.11 
	0.40 
	0.33 
	0.16 
	0.19 
	0.34 
	0.32 
	0.15 

	
	High Speed
	0.07 
	0.31 
	0.31 
	0.32 
	0.06 
	0.42 
	0.34 
	0.18 

	No.4
	Total
	0.13 
	0.33 
	0.35 
	0.19 
	0.24 
	0.31 
	0.28 
	0.17 

	
	Low Speed
	0.25 
	0.30 
	0.34 
	0.11 
	0.38 
	0.26 
	0.21 
	0.15 

	
	Medium Speed
	0.11 
	0.39 
	0.34 
	0.16 
	0.20 
	0.32 
	0.31 
	0.16 

	
	High Speed
	0.07 
	0.29 
	0.32 
	0.33 
	0.06 
	0.39 
	0.36 
	0.20 

	No.5
	Total
	0.13 
	0.33 
	0.35 
	0.19 
	0.23 
	0.32 
	0.29 
	0.16 

	
	Low Speed
	0.26 
	0.28 
	0.34 
	0.12 
	0.37 
	0.25 
	0.23 
	0.15 

	
	Medium Speed
	0.11 
	0.38 
	0.36 
	0.15 
	0.20 
	0.32 
	0.32 
	0.16 

	
	High Speed
	0.07 
	0.33 
	0.34 
	0.27 
	0.06 
	0.43 
	0.36 
	0.16 

	No.6
	Total
	0.13 
	0.34 
	0.36 
	0.18 
	0.22 
	0.33 
	0.30 
	0.15 

	
	Low Speed
	0.25 
	0.30 
	0.35 
	0.10 
	0.36 
	0.28 
	0.22 
	0.14 

	
	Medium Speed
	0.11 
	0.37 
	0.36 
	0.17 
	0.20 
	0.33 
	0.33 
	0.14 

	
	High Speed
	0.06 
	0.31 
	0.35 
	0.27 
	0.06 
	0.41 
	0.36 
	0.17 

	No.7
	Total
	0.13 
	0.35 
	0.33 
	0.19 
	0.22 
	0.32 
	0.28 
	0.18 

	
	Low Speed
	0.26 
	0.30 
	0.33 
	0.11 
	0.35 
	0.25 
	0.21 
	0.19 

	
	Medium Speed
	0.11 
	0.39 
	0.32 
	0.18 
	0.20 
	0.32 
	0.31 
	0.17 

	
	High Speed
	0.06 
	0.34 
	0.34 
	0.25 
	0.06 
	0.43 
	0.35 
	0.17 

	No.8
	Total
	0.12 
	0.34 
	0.33 
	0.21 
	0.22 
	0.32 
	0.27 
	0.19 

	
	Low Speed
	0.23 
	0.29 
	0.34 
	0.13 
	0.35 
	0.23 
	0.18 
	0.24 

	
	Medium Speed
	0.11 
	0.40 
	0.32 
	0.17 
	0.20 
	0.34 
	0.32 
	0.14 

	
	High Speed
	0.06 
	0.32 
	0.32 
	0.30 
	0.05 
	0.42 
	0.33 
	0.20 


Table S3 The ratio of four conditions under RDE test
	No
	Characteristic
	Idle Ratio
	Acceleration Ratio
	Deceleration Ratio
	Cruise Ratio

	
	Unit
	%
	%
	%
	%

	No.1
	Total
	0.03 
	0.35 
	0.33 
	0.28 

	
	Low Speed
	0.05 
	0.37 
	0.36 
	0.22 

	
	Medium Speed
	0.02 
	0.34 
	0.29 
	0.35 

	
	High Speed
	0.01 
	0.33 
	0.27 
	0.38 

	No.2
	Total
	0.08 
	0.31 
	0.31 
	0.31 

	
	Low Speed
	0.09 
	0.32 
	0.33 
	0.27 

	
	Medium Speed
	0.06 
	0.26 
	0.26 
	0.41 

	
	High Speed
	0.03 
	0.34 
	0.28 
	0.34 

	No.3
	Total
	0.10 
	0.30 
	0.34 
	0.26 

	
	Low Speed
	0.11 
	0.31 
	0.34 
	0.24 

	
	Medium Speed
	0.14 
	0.24 
	0.31 
	0.32 

	
	High Speed
	0.03 
	0.33 
	0.36 
	0.28 

	No.4
	Total
	0.05 
	0.33 
	0.30 
	0.31 

	
	Low Speed
	0.07 
	0.35 
	0.32 
	0.25 

	
	Medium Speed
	0.03 
	0.31 
	0.28 
	0.39 

	
	High Speed
	0.01 
	0.30 
	0.26 
	0.43 

	No.5
	Total
	0.05 
	0.34 
	0.30 
	0.30 

	
	Low Speed
	0.07 
	0.36 
	0.31 
	0.26 

	
	Medium Speed
	0.04 
	0.27 
	0.26 
	0.43 

	
	High Speed
	0.03 
	0.35 
	0.30 
	0.32 

	No.6
	Total
	0.05 
	0.35 
	0.31 
	0.29 

	
	Low Speed
	0.07 
	0.36 
	0.33 
	0.24 

	
	Medium Speed
	0.02 
	0.32 
	0.30 
	0.35 

	
	High Speed
	0.02 
	0.32 
	0.28 
	0.38 

	No.7
	Total
	0.03 
	0.35 
	0.32 
	0.30 

	
	Low Speed
	0.04 
	0.36 
	0.33 
	0.26 

	
	Medium Speed
	0.02 
	0.32 
	0.31 
	0.35 

	
	High Speed
	0.02 
	0.32 
	0.30 
	0.37 

	No.8
	Total
	0.06 
	0.37 
	0.29 
	0.28 

	
	Low Speed
	0.09 
	0.39 
	0.31 
	0.21 

	
	Medium Speed
	0.03 
	0.29 
	0.26 
	0.42 

	
	High Speed
	0.01 
	0.35 
	0.25 
	0.40 
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Fig S1. the velocity profiles for the RDE tests
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