Table 1 Design factors and their level

	Design factors: k=2
(reinforcement type)
	Levels:  m=5
(wt.%)

	Short rayon fibres 
	0
	10
	20
	30
	40

	Softwood flour
	0
	10
	20
	30
	40


