Table 1 Measurement point settings in Huanglongxian Village
	Site name
	Space type
	Environmental parameters
	SVF
	Elevation
	Fisheye photos

	A1
	Courtyard space
	Underlying surface: brick and stone
Building orientation: 180 °
	0.928
	[image: ]
	[image: 1]

	A2
	Courtyard space
	Underlying surface: brick and stone
Building orientation: 210 °
	0.817
	[image: ][image: 2]
	[image: 2]

	A3
	Alleyway street space
	Underlying surface: brick and stone
Street width: 12m
	0.934
	[image: ]
	[image: 3]

	A4
	Alleyway street space
	Underlying surface: brick and stone
Street width: 8m
	0.643
	[image: ]
	[image: 4]

	A5
	Square space
	Underlying surface: brick and stone
Square area: 200m2
	0.89
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	[image: 5]

	A6
	Square space
	Underlying surface: brick and stone
Square area: 300m2
	0.802
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	[image: 6]

	A7
	Waterfront space
	Underlying surface: anticorrosive wood
Water area: 0.1hm2
	0.714
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	[image: 7]

	A8
	Waterfront space
	Underlying surface: anticorrosive wood
Water area: 2hm2
	0.775
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Table 2 Measurement point settings in Shishanxia Village
	Site name
	Space type
	Environmental parameters
	SVF
	Elevation
	Fisheye photos

	B1
	Courtyard space
	Underlying surface: brick and stone
Building orientation: 135°
	0.611
	[image: ]
	[image: ]

	B2
	Courtyard space
	Underlying surface: brick and stone
Building orientation: 90°
	0.801
	[image: ][image: 2]
	[image: ]

	B3
	Alleyway street space
	Underlying surface: brick and stone
Street width: 6m
	0.484
	[image: ]
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	B4
	Alleyway street space
	Underlying surface: brick and stone
Street width: 8m
	0.575
	[image: ]
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	B5
	Square space
	Underlying surface: brick and stone
Square area:1150m2
	0.745
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	B6
	Square space
	Underlying surface: anticorrosive wood
Square area:300m2
	0.802
	[image: ]
	[image: ]

	B7
	Waterfront space
	Underlying surface: anticorrosive wood
Water area:1hm2
	0.823
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	B8
	Waterfront space
	Underlying surface: brick and stone
Water area:0.4hm2
	0.523
	[image: ]
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Table 3 Measurement point settings in Huashu Village
	Site name
	Space type
	Environmental parameters
	SVF
	Elevation
	Fisheye photos

	C1
	Courtyard space
	Underlying surface: brick and stone
Building orientation:330°
	0.461
	[image: ]
	[image: ]

	C2
	Courtyard space
	Underlying surface: brick and stone
Building orientation:150°
	0.768
	[image: ][image: 2]
	[image: ]

	C3
	Alleyway street space
	Underlying surface: brick and stone
Street width: 7m
	0.747
	[image: ]
	[image: ]

	C4
	Alleyway street space
	Underlying surface: brick and stone
Street width: 5m
	0.752
	[image: ]
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	C5
	Square space
	Underlying surface: brick and stone
Square area:1200m2
	0.603
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	[image: ]

	C6
	Square space
	Underlying surface: brick and stone
Square area:300m2
	0.959
	[image: ]
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	C7
	Waterfront space
	Underlying surface: anticorrosive wood
Water area:2.5hm2
	0.701
	[image: ]
	[image: ]

	C8
	Waterfront space
	Underlying surface: brick and stone
Water area:0.4hm2
	0.894
	[image: ]
	[image: ]
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