Table 8 Number of sampling filters in the high concentration class of wood dust (>5 mg·m-3) per forest species and operational parameter
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>5mg m-3
	Forest species

	
	X1
	X2
	X3

	
Operating parameters
	Y1
	0
	1
	2

	
	Y2
	1
	1
	3

	
	Y3
	1
	1
	0


Y1=Normal conditions, Y2=Improper maintenance, Y3=Infrequent accelerator,
X1=Fagus sylvatica, X2=Quercus sp., X3=Pinus brutia, 


