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Figure S1. (a) A map showing the location of the study area, (b) excavation of the pit of dimensions 2 m width by 4 m length and 2 m depth, (c) the refill of the pit with the same excavated material and engine oil spillage surface at a depth of 0.3 m from the ground surface, (d) burial of the engine oil with the initial excavated material of the area up to the ground level and, (e) photograph of a standard auger planted into the uncontaminated zone of the study area. 





Table S1:
	Sample ID: 2019 
	Sample ID: 2017 
	Depth
	Description

	EESD1 (C1)
	*
	0-10
	Control 1

	EESD2 (C2)
	*
	42-48
	Control 2

	EESD3 (C4)
	*
	70-80
	Control 4

	EESD4 (T1A)
	EESD9 (T1B)
	0-10
	Above Oil Zone 1

	EESD5 (T2A)
	EESD11 (T2B) 
	42-48
	Above Oil Zone 2

	EESD6 (T3A)
	EESD12 (T3B)
	61-67
	Oil zone

	EESD7 (T4A)
	EESD13 (T4B)
	70-80
	Below oil zone


* Samples were not collected
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