
Highlights

In-plane and out-of-plane permeability test of aramid fiber/glass fiber hybrid fabrics.
The wettability of materials with different hybridization is evaluated by analyzing the dynamic contact angle and surface free energy.

Through analysis, the positive hybrid effect of aramid fiber/glass fiber hybrid fabric permeability is explained

