The solvent method was adopted for grafting modification of recycled PE, and the optimal solvent for grafting was screened by HSPiP software simulation as well as experimental validation, and then combined with the guidance of thermodynamic properties, and the theoretical guidance of the solvent screening process was done.

[bookmark: _GoBack]PE was graft-modified by solution method, and the optimum process conditions were obtained by orthogonal experiments.
