Table 1) Sampling wells and selected geochemical and geophysical features including measured total organic carbon (TOC) and dissolved organic carbon (DOC).
	Sampling well
	Well depth (m)
	Water depth (m)
	Screen interval (m)
	Hydraulic gradient (unitless)
	Hydraulic conductivity
(m s-1)
	TOC
(mg L-1 )
	DOC
(mg L-1 )
	POC
(mg L-1 )

	Well 1
	9.0
	3.69
	5.2 – 8.1
	0.0143
	6.10E-04
	12.4±0.21
	11.5±0.06
	0.9

	Well 2
	7.2
	4.58
	3.0 – 6.0
	0.0143
	4.50E-04
	3.00±0.14
	2.97±0.06
	0.03

	Well 3
	4.5
	1.60
	1.9 – 3.9
	0.0185
	4.50E-04
	5.13±0.21
	4.97±0.12
	0.16


















[bookmark: _Hlk151997087]Table 2) LDPE-based freely dissolved concentrations (μg L-1) measured at 80 d and total dissolved concentrations (DOC-bound + freely dissolved) in triplicate filtered water (μg L-1) samples.   Total dissolved samples were collected three days prior to deployment of passive samplers.
	PAHs
	Well 1

	Well 2
	Well 3

	
	Ctotal
	Cw
	Ctotal
	Cw
	Ctotal
	Cw

	[bookmark: _Hlk151998038]Naphthalene
	143.33±11.55
	0.05±0
	0.29±0.14
	nd
	20.67±2.31
	0.05±0.01

	Acenaphthylene
	19.67±2.31
	0.19±0.14
	1.01±0.08
	0.01±0
	20.67±2.52
	0.28±0.01

	Acenaphthene
	4.77±0.78
	0.51±0.58
	53.33±3.06
	0.03±0.02
	756.67±132.04
	28.32±1.08

	Fluorene
	4.7±0.62
	0.43±0.31
	0.45±0.06
	0.01±0
	176.67±30.55
	0.45±0.16

	Phenanthrene
	6.77±0.93
	0.06±0.02
	0.08±0.01
	nd
	20.67±4.51
	0.03±0.01

	Anthracene
	1.63±0.21
	0.04±0.02
	0.26±0.03
	0.002±0
	5.1±0.61
	0.03±0.01

	Fluoranthene
	8.13±1.61
	0.51±0.11
	2.87±0.32
	0.01±0
	3.63±0.38
	0.02±0

	Pyrene
	4.5±0.96
	0.25±0.04
	1.37±0.15
	0.01±0
	1.47±0.15
	0.01±0

	Benzo(a)anthracene
	0.97±0.32
	0.002±0
	0.01±0
	nd
	0.01±0
	nd

	Chrysene
	0.78±0.26
	0.004±0
	0.03±0.01
	0.0001±0
	0.01±0
	nd

	Benzo(b)fluoranthene
	0.39±0.16
	0.0001±0
	nd
	nd
	nd
	nd

	Benzo(k)fluoranthene
	0.38±0.15
	0.0001±0
	nd
	nd
	nd
	nd

	Benzo(a)pyrene
	0.59±0.25
	0.0002±0
	nd
	nd
	nd
	nd

	Indeno(1,2,3-cd)pyrene
	0.17±0.09
	nd
	nd
	nd
	nd
	nd

	Dibenzo(a,h)anthracene
	0.05±0.03
	nd
	nd
	nd
	nd
	nd

	Benzo(ghi)perylene
	0.18±0.09
	nd
	nd
	nd
	nd
	nd




Table 3.  Accumulated PAH concentrations (µg/PE) in LDPEs exposed to groundwater wells 1, 2, and 3 across two to six sampling times.
	PAHs
	Well 1
	Well 2
	Well 3

	
	42 d
	80 d
	42 d
	80 d
	14 d
	28 d
	42 d
	56 d
	70 d
	80 d

	Naphthalene
	0.02±0.01
	0.03±0
	< 0,01
	< 0,01
	0.075±0.01
	0.03±0.01
	0.02±0
	0.02±0.01
	0.03±0.01
	0.03±0.01

	Acenaphthylene
	0.24±0.11
	0.25±0.2
	0.01±0
	0.02±0
	0.503±0.05
	0.47±0.04
	0.46±0.02
	0.39±0.08
	0.38±0.07
	0.36±0.01

	Acenaphthene
	0.35±0.08
	0.98±1.12
	0.03±0.01
	0.09±0.03
	54.83±12.2
	56.67±4.16
	53.33±4.73
	51.67±7.51
	55.07±10.1
	55.93±2.09

	Fluorene
	0.35±0.06
	1.23±0.89
	< 0,01
	0.03±0.01
	2.55±0.75
	2.00±0.56
	1.93±0.4
	1.63±0.55
	1.59±0.8
	1.51±0.36

	Phenanthrene
	0.5±0.19
	1.23±0.12
	< 0,01
	< 0,01
	0.29±0.11
	0.32±0.09
	0.29±0.1
	0.31±0.12
	0.32±0.14
	0.29±0.13

	Anthracene
	0.47±0.21
	0.73±0.07
	0.01±0
	0.02±0
	0.09±0.02
	0.16±0.09
	0.12±0.03
	0.19±0.07
	0.28±0.08
	0.29±0.07

	Fluoranthene
	16.00±0
	23.22±4.69
	0.07±0.03
	0.28±0.06
	0.24±0.11
	0.43±0.05
	0.45±0.07
	0.55±0.11
	0.66±0.09
	0.77±0.02

	Pyrene
	8.77±0.38
	13.03±2.16
	0.15±0.02
	0.28±0.01
	0.14±0.05
	0.23±0.02
	0.25±0.02
	0.29±0.06
	0.35±0.04
	0.40±0.03

	Benzo(a)anthracene
	0.16±0.01
	0.29±0.05
	< 0,01
	< 0,01
	< 0,01
	< 0,01
	< 0,01
	< 0,01
	< 0,01
	< 0,01

	Chrysene
	0.14±0.02
	0.48±0.1
	< 0,01
	< 0,01
	< 0,01
	< 0,01
	< 0,01
	< 0,01
	< 0,01
	< 0,01

	Benzo(b)fluoranthene
	< 0,01
	0.03±0.01
	< 0,01
	< 0,01
	< 0,01
	< 0,01
	< 0,01
	< 0,01
	< 0,01
	< 0,01

	Benzo(k)fluoranthene
	< 0,01
	0.02±0
	< 0,01
	< 0,01
	< 0,01
	< 0,01
	< 0,01
	< 0,01
	< 0,01
	< 0,01

	Benzo(a)pyrene
	< 0,01
	0.05±0.02
	< 0,01
	< 0,01
	< 0,01
	< 0,01
	< 0,01
	< 0,01
	< 0,01
	< 0,01

	Indeno(1,2,3-cd)pyrene
	< 0,01
	< 0,01
	< 0,01
	< 0,01
	< 0,01
	< 0,01
	< 0,01
	< 0,01
	< 0,01
	< 0,01

	Dibenzo(a,h)anthracene
	< 0,01
	< 0,01
	< 0,01
	< 0,01
	< 0,01
	< 0,01
	< 0,01
	< 0,01
	< 0,01
	< 0,01

	Benzo(ghi)perylene
	< 0,01
	< 0,01
	< 0,01
	< 0,01
	< 0,01
	< 0,01
	< 0,01
	< 0,01
	< 0,01
	< 0,01










