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Table S1. Parameters and their levels based on DEP.
	
Independent variable
	
Factor
	Variable levels

	
	
	-α
	-1
	0
	+1
	+α

	Fe/Li molar ratio [-]
	A
	0.50
	1.01
	1.75
	2.49
	3.00

	HCl concentration [M]
	B
	0
	0.10
	0.25
	0.40
	0.50

	TBP vol percent [%]
	C
	10.00
	26.22
	50.00
	73.78
	90.00
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Fig. S1. UV-VIS spectra for determination of extraction complex wavelengths.

[image: ]
[bookmark: _GoBack]  Fig. S2. Response sensitivity to major parameters (A, B, and C: Mean).         
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