Role of cow dung and sawdust during the bioconversion of swine waste through the rotary drum composting process
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	Figure A1. FTIR Spectroscopy a) RDC1 and b) RDC2
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Table A1. Correlation between the parameters of RDC1
	 
	Duration (Day)
	Temperature
	Moisture content 
	EC  
	pH 
	Volatile solids
	TOC
	TKN 
	C/N 
	Ammonia
	C02 Evolution
	Potassium 

	Duration (Day)
	1.00
	 
	 
	 
	 
	 
	 
	 
	 
	 
	 
	 

	Temperature
	-0.55
	1.00
	 
	 
	 
	 
	 
	 
	 
	 
	 
	 

	Moisture content 
	-0.93
	0.34
	1.00
	 
	 
	 
	 
	 
	 
	 
	 
	 

	EC  
	0.94
	-0.61
	-0.89
	1.00
	 
	 
	 
	 
	 
	 
	 
	 

	pH 
	0.87
	-0.33
	-0.98
	0.81
	1.00
	 
	 
	 
	 
	 
	 
	 

	Volatile solids
	-0.98
	0.57
	0.89
	-0.92
	-0.82
	1.00
	 
	 
	 
	 
	 
	 

	TOC
	-1.00
	0.58
	0.91
	-0.94
	-0.85
	0.99
	1.00
	 
	 
	 
	 
	 

	TKN 
	0.95
	-0.70
	-0.79
	0.92
	0.70
	-0.96
	-0.97
	1.00
	 
	 
	 
	 

	C/N 
	-0.97
	0.64
	0.88
	-0.97
	-0.80
	0.97
	0.98
	-0.98
	1.00
	 
	 
	 

	Ammonia
	-0.99
	0.56
	0.92
	-0.96
	-0.85
	0.98
	0.99
	-0.96
	0.98
	1.00
	 
	 

	C02 Evolution
	-0.98
	0.44
	0.97
	-0.92
	-0.91
	0.95
	0.96
	-0.88
	0.94
	0.97
	1.00
	 

	Potassium 
	0.99
	-0.55
	-0.94
	0.93
	0.89
	-0.98
	-0.99
	0.94
	-0.97
	-0.99
	-0.98
	1.00











Table A2. Correlation between the parameters of RDC2
	 
	Duration (Day)
	Temperature
	Moisture content 
	EC  
	pH 
	Volatile solids
	TOC
	TKN 
	C/N 
	Ammonia
	C02 Evolution
	Potassium 

	Duration (Day)
	1.00
	 
	 
	 
	 
	 
	 
	 
	 
	 
	 
	 

	Temperature
	-0.66
	1.00
	 
	 
	 
	 
	 
	 
	 
	 
	 
	 

	Moisture content 
	-0.84
	0.29
	1.00
	 
	 
	 
	 
	 
	 
	 
	 
	 

	EC  
	0.93
	-0.67
	-0.85
	1.00
	 
	 
	 
	 
	 
	 
	 
	 

	pH 
	0.98
	-0.68
	-0.84
	0.97
	1.00
	 
	 
	 
	 
	 
	 
	 

	Volatile solids
	-0.98
	0.55
	0.92
	-0.93
	-0.96
	1.00
	 
	 
	 
	 
	 
	 

	TOC
	-0.97
	0.55
	0.92
	-0.92
	-0.96
	1.00
	1.00
	 
	 
	 
	 
	 

	TKN 
	0.97
	-0.71
	-0.76
	0.94
	0.96
	-0.92
	-0.91
	1.00
	 
	 
	 
	 

	C/N 
	-0.99
	0.65
	0.87
	-0.97
	-0.98
	0.98
	0.97
	-0.97
	1.00
	 
	 
	 

	Ammonia
	-0.97
	0.55
	0.93
	-0.95
	-0.96
	1.00
	0.99
	-0.92
	0.98
	1.00
	 
	 

	C02 Evolution
	-0.97
	0.59
	0.93
	-0.95
	-0.97
	0.99
	0.98
	-0.91
	0.97
	0.99
	1.00
	 

	Potassium 
	0.94
	-0.44
	-0.94
	0.89
	0.90
	-0.98
	-0.98
	0.86
	-0.94
	-0.98
	-0.96
	1.00
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